Table 14 - Data for Terminal Stations

(Based on reference 4)

Active failure rate of a breaker (failure/year)	=	0.0066

Passive failure rate of a breaker (failure/year)	=	0.0005

Maintenance rate of a breaker (outages/year)	=	0.2

Maintenance time of a breaker (hours)	=	108

Switching time - one or more components (hours)	=	1.0